**MYUNG JIN SHIPPING CO., LTD.**

RM 301, 988-5, GOHYUN DONG, GEOJE, GYEONG NAM, KOREA

FLAT BARGE ‘ POS 25000’



|  |  |
| --- | --- |
| GENERAL |  |
| Vessel’s name | POS 25000 |
| Builder | ForceTEC Corporation |
| Year Built  | APRIL 2009 |
| Type | Flat Barge |
| Classification Society | K.R(Class No. 0966705) |
| Flag | KOREA |
| IMO NO /Official NO / Call Sign | - / MSB-097157 / - |
| Navigation Area | Great Coastal |
|  |  |
| DIMENSIONS |  |
| LOA | 95.04 M |
| Breadth (MLD) | 36.00 M |
| Depth (MLD) | 6.50 M |
| GRT / NRT | 6,190T / 1,857T |
| Dead Weight | 12,500T |
|  |  |
| Tank Capacity |  |
| IFO | - |
| MGO | 12.0 k/l |
| L.O |  |
| Ballast Capacity | 2,000㎥/hr x 3EA = 6,000㎥/hr |
| Fresh Water |  |
|  |  |
| PERFORMANCE |  |
| E/R MACHINERY |  |
| Main Generator Engine Power | 504KW \* 1 Set |
| Aux’ Generator Engine Power | 24KW \* 1Set |
| G.S & Fire Pump Capacity | 90㎥/hr \* 1Set |
| BILGE & G.S Pump Capacity | 90㎥/hr \* 1Set |
| Ventilation Fan | 2 set |
| F.W PUMP | 1 SET (HANIL) |
| Oily Water Separator | 1Set (1㎥/hr \* 15ppm) |
|  |  |
| Deck Machinery |  |
| Anchor & Chan | 3,540Kg \* 54￠\*9Shot \* 2Set |
| Windless | 9m / min \* 13.0Ton 2Set |
| Windless Hyd. Pump \* Motor | 440V \* 60Hz \* 37.0 Kw |
| MOORING WINCH | 2 Set(10M/min \* 6.0 TON) |
|  |  |
| Communication |  |
| HAND V.H.F | ICOM \* 2Set |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

Particulars are given entirely without warranty as to correctness and interested parties must satisfy themselves by inspection of the vessel.